Canon BJ-10e - Paper Going Through Printer Bu

DocumentID: 609649
Revision Date: 29-Feb-96 1:34:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: FYI: A customer was able to successfully print at DOS, however, in WordPerfect the paper rolled through the printer without printing. Changing all the dip switches to Off, except for 10, corrected the problem. When switch 10 is On, the printer is in Mode 2.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.