Labels - Setting Right Margin To 0" Through P

DocumentID: 610885
Revision Date: 29-Feb-96 1:34:37 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is not able to set a 0" right margin when printing labels to a Roland Raven PR-9101 (Panasonic KX-P1180) printer. Solutions: The customer can change the minimum margin settings by doing the following in the PTR Program: 1. Enter the PTR Program and retrieve the .PRS file. Press Enter on the printer. 2. Move to Miscellaneous Numbers and press Enter. 3. Move to Minimum Right Margin and change it from 0.5 to 0. 4. Exit and save. NOTE: This should only be done on wide-carriage emulations of the Roland Raven PR-9101 (Panasonic KX-P1180).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.