NEC Silentwriter Model 95 - Changing To HP II

DocumentID: 642233
Revision Date: 29-Feb-96 8:18:43 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: You can place the NEC Silentwriter Model 95 PostScript printer in HP III emulation mode by following the steps below: 1. Press the On-Line button until the printer window reads Not Ready 2. Press the Menu button (Emulation will display in the window) 3. Press the Select button (PostScript will display in the window) 4. Press the Previous button (HP LaserJet III will display in the window) 5. Press the Select button to select the emulation 6. Press the On-Line button This will then reset the printer to the HP III mode.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.