QMS PS 820 Turbo Printer - General Informatio

DocumentID: 646842
Revision Date: 29-Feb-96 8:19:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The QMS PS 820 Turbo printer supports the Adobe PostScript page description language. It also includes HP LaserJet Plus and HP-GL emulations for non-PostScript applications. This printer uses the Canon TX print engine and has a rated printing speed of eight pages per minute. This printer includes dual 200-sheet input paper trays and uses QMS ASAP (Advanced System Architecture for PostScript) technology and a 68020 microprocessor for faster "first page out" performance. The QMS PS 820 Turbo printer comes with 39 resident Adobe PostScript typefaces (all of which can be scaled from 4 points upward), 2 megabytes of RAM standard, and PS Executive Series Utilities software (which allows users to perform functions such as port setup, memory allocation, emulation switching, and printer alignment). This printer instantly connects into most environments, including IBM PCs, Apple Macintosh computers, and most mini and mainframes. It also includes a SCSI interface to which users can attach up to seven external hard drives for storage of downloadable typefaces, emulations, and PostScript programs.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.