Printing To The AS/400 With User Contributed

DocumentID: 638055
Revision Date: 29-Feb-96 3:04:49 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer wanted to utilize a 3812 IBM printer that was connected to an AS400 mini. They had PCSUPPORT (a DOS to IBM SCS print queue) running on a network. WordPerfect 5.1 has a user contributed driver, SCS 381x, that will utilize such a link. Thus, WP 5.1 users can print to the AS/400. In this case the printer was hooked up via Twin Ax which is one of three possible ways (Coax, Twin Ax, or Parallel) to connect to an AS/400. *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.