Large Graphic Prints On Four Pages On Banyan

DocumentID: 654162
Revision Date: 29-Feb-96 8:29:29 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A PCX graphic image printed at high quality through a Banyan Vines 4.0.5 network was split into four pages. First, a banner page printed followed by the first quarter of the graphic, then a second banner page printed followed by the second quarter of the graphic, and so forth. The problem also occurred when printing other graphics or large line draw files. When the print quality was set to medium or draft, or when printing to the local printer the problem did not occur. The problem was corrected by following the steps below to increase the network timeouts. 1. Run the Banyan SETPRINT.EXE utility 2. Select the port 3. Select Modify Printer Setup

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.