The Macintosh Apple Family Of Computers

DocumentID: 603380
Revision Date: 29-Feb-96 1:29:45 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The following list is of different models of the Macintosh Apple line of computers and some general information about each model. Computer Model: 128K Intro Year: 1984 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 128K-128K Data Path: 16-bit Floppy Drive: 400K Hard Drive: None Math Coproc: None Expan Slots: None Computer Model: 512K Intro Year: 1984 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 512K-512K Data Path: 16-bit Floppy Drive: 800K Hard Drive: None Math Coproc: None Expan Slots: None Computer Model: 512 KE Intro Year: 1986 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 512K-1024K Data Path: 16-bit Floppy Drive: 800K Hard Drive: None Math Coproc: None Expan Slots: None Computer Model: Plus Intro Year: 1986 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 1M-4M Data Path: 16-bit Floppy Drive: 800K Hard Drive: External Avail Math Coproc: None Expan Slots: None Computer Model: SE Intro Year: 1987 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 1M-4M Data Path: 16-bit Floppy Drive: 800K Hard Drive: 20M Math Coproc: None Expan Slots: None Computer Model: SE {1988} Intro Year: 1988 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 1M-4M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 20M Math Coproc: None Expan Slots: None Computer Model: Mac II Intro Year: 1987 CPU Chip: 68020 Chip Speed: 16 MHz Min-Max RAM: 2M-32M Data Path: 32-bit Floppy Drive: 800K Hard Drive: 40M Math Coproc: # 68881 Expan Slots: 6 Computer Model: Mac IIX Intro Year: 1988 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 2M-32M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 6 Computer Model: SE/30 Intro Year: 1989 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 1M-32M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 1 Computer Model: Classic Intro Year: 1990 CPU Chip: 68000 Chip Speed: 8 MHz Min-Max RAM: 1M-4096K Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: None Computer Model: Classic II Intro Year: 1991 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 2M-10M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: None Computer Model: Mac IICX Intro Year: 1989 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 2M-32M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 3 Computer Model: Mac IICI Intro Year: 1989 CPU Chip: 68030 Chip Speed: 25 MHz Min-Max RAM: 4M-32M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 3 Computer Model: Mac IIFX Intro Year: 1990 CPU Chip: 68030 Chip Speed: 40 MHz Min-Max RAM: 4M-32M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: # 68882 Expan Slots: 6 Computer Model: Mac IILC Intro Year: 1990 CPU Chip: 68020 Chip Speed: 16 MHz Min-Max RAM: 2M-10M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: 1 Computer Model: MacIISI Intro Year: 1990 CPU Chip: 68030 Chip Speed: 20 MHz Min-Max RAM: 2M-17M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: Avail Expan Slots: 1 Computer Model: Quadra 700 Intro Year: 1991 CPU Chip: 68040 Chip Speed: 25 MHz Min-Max RAM: 4M-20M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: Integrated Expan Slots: 2 Computer Model: Quadra 900 Intro Year: 1991 CPU Chip: 68040 Chip Speed: 25 MHz Min-Max RAM: 4M-64M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 160M Math Coproc: Integrated Expan Slots: 5 Computer Model: Mac IILC Intro Year: 1992 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 2M-64M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: 1 Computer Model: Quadra 950 Intro Year: 1992 CPU Chip: 68040 Chip Speed: 33 MHz Min-Max RAM: 8M-64M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 160M Math Coproc: Integrated Expan Slots: 5 Computer Model: Mac IIVX Intro Year: 1992 CPU Chip: 68030 Chip Speed: 32 Mhz Min-Max RAM: 4M-20M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 3 Computer Model: Portable Intro Year: 1989 CPU Chip: 68000 Chip Speed: 16 MHz Min-Max RAM: 1M-9M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: 0 Computer Model: PowerBook 100 Intro Year: 1991 CPU Chip: 68000 Chip Speed: 16 MHz Min-Max RAM: 2M-8M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 20M Math Coproc: None Expan Slots: 0 Computer Model: PowerBook 140 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 2M-8M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 20M Math Coproc: None Expan Slots: 0 Computer Model: PowerBook 145 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 25 MHz Min-Max RAM: 2M-8M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 20M Math Coproc: None Expan Slots: 0 Computer Model: PowerBook 160 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 25 MHz Min-Max RAM: 2M-14M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 20M Math Coproc: None Expan Slots: 0 Computer Model: PowerBook 170 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 25 MHz Min-Max RAM: 4M-8M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: # 68882 Expan Slots: 0 Computer Model: PowerBook 180 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 33 MHz Min-Max RAM: 4M-14M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: # 68882 Expan Slots: 0 Computer Model: PB Duo 210 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 25 MHz Min-Max RAM: 4M-25M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: Avail Expan Slots: 0 Computer Model: PB Duo 230 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 33 MHz Min-Max RAM: 4M-24M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: Avail Expan Slots: 0 Computer Model: Performa 200 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 4M-10M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: None Expan Slots: 0 Computer Model: Performa 400 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 4M-10M Data Path: 16-bit Floppy Drive: 1.44 M Hard Drive: 40 M Math Coproc: None Expan Slots: 1 Computer Model: Performa 600 Intro Year: 1992 CPU Chip: 68030 Chip Speed: 32 MHz Min-Max RAM: 4M-20M Data Path: 32-bit Floppy Drive: 1.44M Hard Drive: 80M Math Coproc: Avail Expan Slots: 3 Computer Model: *Mac IIVI Intro Year: 1992 CPU Chip: 68030 Chip Speed: 16 MHz Min-Max RAM: 4M-20M Data Path: 16-bit Floppy Drive: 1.44M Hard Drive: 40M Math Coproc: Avail Expan Slots: 3 * International release only. Other configurations are possible than those detailed here. Examples: Cache Memory, Video Memory, ability to accept CD ROM drive, etc.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.