POSTNET Macro Prints Barcodes Too Short On HP

DocumentID: 610357
Revision Date: 29-Feb-96 1:34:30 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The POSTNET barcode macro prints the barcodes too short on an HP LaserJet III PostScript printer. The barcodes print properly if the user does not use the PostScript card. Solutions: The problem occurs because of the minimum right margin allowed on the printer. The customer can either print the barcode above the address, or edit the .PRS file and change the minimum right margin to .25" or less. How/Why: Envelopes print landscape. When a customer prints in landscape mode, the minimum right margin becomes the minimum bottom margin.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.