Print - "Error 18" When Using Glyphix And A P

DocumentID: 646761
Revision Date: 29-Feb-96 8:19:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The message "Error 18" appeared when printing. The customer was using Glyphix fonts, a PostScript printer, and printing through the LPT1 port. The user eliminated the error by loading a Glyphix TSR named LPT3TO1.EXE. Loading WP without Glyphix, or using a DOS MODE command to redirect the LPT1 port to COM2 can also eliminate the printing error. Note: LPT3TO1 can be found in the GLSFONTS directory. It allows users to change the port of the PostScript printer to LPT3, yet have the printer physically attached to LPT1. To use the LPT3TO1.COM utility, the customer would type LPT3TO1 at the Glyphix directory prior to entering WordPerfect. The customer then enters WP using GX.EXE. The user should then change the port from LPT1 to LPT3. *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.