Toshiba P351C - Only Printing On One Band Of

DocumentID: 641515
Revision Date: 29-Feb-96 8:18:37 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The Toshiba P351C was printing on only one band of the black ribbon thus wearing out only one band on the ribbon and wasting the other three. Solutions: The user referred to the Select Auto Ribbon Band Shift section in the Toshiba manual and made the following changes in the PTR Program to correct his problem: 1. Retrieve the .PRS file. 2. Press Enter on Initialize and Reset. 3. Highlight Initialize at Start of Page. 4. Press the Right Arrow key to go to the Expression box. 5. Type in [27,102] (The code specified in the Toshiba manual.) 6. Exit out and resave the file.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.