Diablo 635 Printing With A Sheet Feeder

DocumentID: 634212
Revision Date: 29-Feb-96 3:03:35 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The Diablo 635 with a parallel interface has four dip switches. Switch number one controls whether there is a sheet feeder or whether it is tractor feed and manually fed. If switch one is ON, the printer understands that there is a sheet feeder. One customer using the Diablo sheet feeder switched dip switch number one to OFF (as suggested in PRHELP). With this switch off the printer would not print from WordPerfect or from DOS. A paper out signal was given. But turning the switch ON allowed proper printing from DOS and from WordPerfect.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.