NEC Spinwriter Elf 360 Bold PS Wheel

DocumentID: 647554
Revision Date: 29-Feb-96 8:19:22 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: When using the Bold PS wheel on the NEC Spinwriter Elf 360 the letters may run together or the word may not justify correctly. The following seems to work in fixing these problems: 1. Enter the PTR program and retrieve the WPDW1.ALL file. Highlight the printer name and press Enter to edit. 2. Cursor to Horizontal Motion and pressed enter. Mark HMI Only and press Enter to edit this option. Enter [27]"]"SENDLO(HS+64) for Set HMI; 15 (without brackets) for MAX UNITS; [8] for Perform Back Space; [13] for Perform Carriage Return; and NO for Auto Line Feed on Carriage Return. 3. Press F7 to return to the main menu. Cursor to the option for Fonts and press Enter. Highlight *NEC 8830 and press Enter and then press Enter on Bold PS. Cursor to Size and Spacing and press Enter. Select the Proportional Spacing Table option (at the bottom of screen) and press Enter. 4. Cursor to NEC Elf BOLD and type an * then press Enter. Move to the capitol L, press the right arrow to go to the Adjust Value and change it from -2 to 0. Move to the small m and change the value from 1 to 2. 5. Press Alt-F7 to exit the PTR program, saving the file as you do so. Enter WordPerfect and Update the Printer file (Shift-F7, S, 7).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.