Accessing Different Bins With UDP TurboScript

DocumentID: 601663
Revision Date: 29-Feb-96 1:28:45 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Can the UDP TurboScript II/III PostScript cartridge access different bins on an HP LaserJet IID or IIID? Solutions: According to UDP Technical Support these cartridges can only access a single bin on the printer. You can change the tray on the printer if you remove the PostScript cartridge and turn on the printer, then set the printer menu to the tray you need. To do this follow the steps below: 1. Turn the printer On without the cartridge inserted 2. Press On Line 3. Press Menu 4. Continue to press Menu until the printer reads TRAY= 5. Use the +/- key to change to the tray you need 6. Press the Enter button on the printer to save the change 7. Press On-Line 8. Turn the printer off then on again with the Postscript cartridge Inserted

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.