Toshiba P321SL/P341SL Graphics Not Printing I

DocumentID: 644787
Revision Date: 29-Feb-96 8:19:01 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The user's Toshiba P321SL prints a graphic that is supposed to be on the right hand side, on the left hand side of the page. If the printer is in IBM mode with the IBM Proprinter selected, it works properly. Solutions: Do the following to fix the problem: 1. Type PTR at the DOS prompt and retrieve the *.PRS file. 2. Press Enter on the Printer Name. 3. Press Enter on Horizontal Motion. 4. Press Enter on Relative Horizontal Motion. 5. Press the right arrow key to move to the expression box, next to Move Forward. 6. Press Shift-F9 for function variables. Rename hs1 to hs2. Exit back to the expression box for move forward and change the hs1 variables to hs2. 7. Press F7 to save the file. The problem was an Integer variable called hs1 and a function variable called hs1. For Move Forward we wanted to input the Function variable and instead the Integer value was being sent. This is what was causing the incorrect positioning. This is a Problem with most Toshiba SL (IBM2) drivers. The Toshiba SL (USA) drivers did not have this error.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.