Duplexing And Multiple Copies With Odd Number

DocumentID: 604203
Revision Date: 29-Feb-96 1:30:31 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Duplex forms should not be defined unless a duplex printer is being used. If a customer does not have a duplex printer and selects a duplex Paper Size/Type in the document, a blank page will be ejected from the printer. This happens only when Multiple Copies (Shift-F7, 5) is selected, and when there are an odd number of pages in the document. When a document has an odd number of duplex pages and Multiple Copies is selected, WordPerfect will send an extra form feed to the printer at the end of the last page so the page can be ejected. This is so the first page of the next print job will not print on the back of the last page of the previous print job.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.