Fujitsu RX7100 Printer - Printing Envelopes

DocumentID: 645157
Revision Date: 29-Feb-96 8:19:03 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: How should envelopes be set up for the Fujitsu RX7100 printer? Solutions: Envelopes for the Fujitsu printers can be set up to print manually or continuously. For manually fed envelopes: 1. Use the regular method of setting up envelopes. 2. The envelope must be placed in the sliding paper guide slots, similar to the ones found on an HP Series II. The flap faces down and left. The envelope must then be placed so the edge going into the printer sets into place. Then as the printer pulls the envelope, the envelope must sometimes be guided as to be able to feed properly into the printer. For continuously fed envelopes: 1. Set up a Paper Size/Type called Envelope, size 9.5"x4", with a location of Bin 2. 2. Insure that the sheet feeder is defined as Fujitsu RX7100 (SF). 3. Create a document using the Envelope Paper Size/Type that was just created for Bin 2. 4. Print the document. 5. After WordPerfect sends the print job, the printer will respond with a message, FEED LEGAL INTO BIN 2. 6. At the printer, change the menu setting for Bin 2 paper type, to legal. 7. Turn the printer off, then on again. 8. Resend the envelope print job. It then prints continuously from the printer.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.