Blank Pages Between Printed Pages - Changes I

DocumentID: 601300
Revision Date: 29-Feb-96 1:28:39 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer would get a blank page between printed pages on an Epson MX-80 Graftrax printer. The problem was corrected by doing the following: 1. Enter the PTR Program 2. Press Shift-F10, Shift-F5, go to the end of filename, delete .ALL and type .PRS 3. Press Enter, put cursor under printer filename and press Enter as many times as it takes to bring the printer name into the box 4. Press Enter 5. Press Enter on Initialize and Reset 6. Delete expressions next to the following: Reset/Advance at End of Page, Printer Auto Page Advance, Set Page Length 7. Exit out of the PTR Program, save and replace file. The Epson MX-80 has many different ROM versions. Epson does not even have a comprehensive list of all of them and what they do. The above steps may or may not work on a particular printer.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.