Labels - Prompting For Manual Feed On Dot-Mat

DocumentID: 604635
Revision Date: 29-Feb-96 1:30:38 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer was prompted to press G to continue for each label when printing 3.5" x 1" labels on a dot-matrix printer. The problem was corrected by changing the location in the [ALL OTHERS] form to Continuous. Another customer receiving the message "Press Shift-f7, 4 To Resume Printing" changed the Prompt To Load to No and the location to Continuous for the [ALL OTHERS] definition in the paper size/type screen to correct the problem.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.