HP LaserJet III - Supported Envelope Sizes Wi

DocumentID: 609080
Revision Date: 29-Feb-96 1:33:57 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The HP 92297F envelope tray, most often used with the HP LaserJet III printers, supports the following envelope sizes: COM 10 envelope (9" x 4"), Monarch/Executive Size envelope (3.875" x 7.5"), DL (22cm x 11cm") and C5 (22.9cm" x 16.2cm"). Printing with any other envelope sizes will have to be done through the manual feed slot. The paper size for monarch must be entered as 7.5" x 3.875"; it will round up to 3.88". If you enter 3.88" as the size originally, a PC LOAD LEGAL message will display on the printer. If you create the form size using the Other option and then type 7.5" x 3.875" for height, the printer will say PC LOAD MONARCH, but if the envelope tray is already inserted into the printer, it will print. This information also applies to the HP LaserJet Series II, HP LaserJet IID, IIID, and IIISi printers.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.