HP LaserJet 4 And Odd Sized Envelopes

DocumentID: 668681
Revision Date: 29-Feb-96 8:50:09 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: When printing odd sized envelopes to an HP LaserJet 4 using the Auto Envelope Feeder, the printer pulls paper from the Paper Cassette. Solutions: To use odd sized envelopes, the user must place the envelopes in the MP tray and specify the location as the MP tray. Causes: The HP Auto Envelope Feeder is designed to allow only certain form sizes. These include Commercial #10, #7 3/4 (Monarch), DL, C5, and B5 envelope sizes. If the form is not one of the predefined forms, the paper will pull from the paper tray.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.