Epson MX-80 "FT" Defined As Graftrax Underlin

DocumentID: 645975
Revision Date: 29-Feb-96 8:19:10 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The Epson MX-80 "FT" printer defined as the Epson MX-80 Graftrax will only print dashed underline, instead of solid. I know that it is dashed on the printer test, but the user can get it solid with Microsoft Windows Write and Deskmate Text (Tandy). Solutions: If the user has the vanilla Epson MX-80 (F/T) printer, we use the underline character in that driver. This character will not connect from cell to cell and cannot be adjusted since the smallest motion is the space. If they have the Type III or Graftrax printer they should use one of those drivers which may work better. I have used the best underline that we could get from the printers that we have for development. The other programs may be using graphics to create a solid underline.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.