HP LaserJet III - Reducing Minimum Margins Ca

DocumentID: 636690
Revision Date: 29-Feb-96 3:04:21 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Reducing the minimum margins for an HP LaserJet III printer driver using the PTR Program causes words to overprint or graphics border lines (like in tables) to overprint the text. Solutions: If you use the current left minimum margin of a HP LaserJet III printer, the margin will read .29". Even though the margin reads .29", WordPerfect 5.1 for DOS does not tell the printer to position over .29" but gives it a horizontal position of 0. This is because the starting position (position 0) of the cursor is .29" from the edge of the paper. You can't force the printer to print at .25" if its starting point is at .29". After decreasing the minimum margin using the PTR Program, overprinting can occur.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.