Okidata ML 390/391 - General Information

DocumentID: 647086
Revision Date: 29-Feb-96 8:19:19 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The Okidata ML 390/391 has two different modes of operation; IBM and Epson. The WordPerfect driver for the 391 is written for the printer in Epson mode. If users have other programs that require the printer to be in IBM mode, then the user should select the IBM X24 printer driver. Customers can change the printer modes by taking the printer off-line, pressing the MODE button on the front of the printer, pressing the GROUP button to move to the Emulation Mode, then pressing the SET button to switch between IBM and Epson. The following is general information regarding the Okidata ML 390/391 printer: 1. If the customer wants to use this printer in IBM mode, have them use the IBM Proprinter X24 driver. 2. Odd sizes of paper work better after the 04/27/91 release of the printer drivers. 3. Line Draw and graphics will work with Pica Compressed fonts with drivers after 04/27/91. 4. The 12/22/88 release of the printer driver fixed underline problems with proportionally spaced fonts. 5. This printer can use font cartridges. Have the customer use the Additional driver if he has a font cartridge. *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.