Displaying Bold & Underline W/ Western Digita

DocumentID: 601151
Revision Date: 29-Feb-96 1:28:37 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: FYI: Executing the following commands at a DOS prompt enabled the display of both underline and bold with a Western Digital (Paradise) VGA1024 graphics card: CLS VGA1024 HERC0 CD WP51 WP VGA1024 VGA MAIN The above commands will work if the customer has a Western Digital (or Paradise) super VGA graphics card and the VGA1024 utility provided by Western Digital. This should work with any monitor. The customer was using the NEC 3D monitor and with a 386/33 MHz computer. After entering the above commands in a batch file, the user entered WP and selected a Hercules monochrome driver for the Graphics Screen Type and auto-selected the Text Screen Type. A similar solution can be found for most Graphics cards that come with a utility to change the graphics card mode to a Hercules emulation before starting WP and then back to VGA mode when exiting WP (which is all this batch file really does.)

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.