NEC Pinwriter P5300 - Small Paper Sizes Not P

DocumentID: 603724
Revision Date: 29-Feb-96 1:30:25 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using the NEC Pinwriter P5300. When printing a form that is not wide enough to cover the center of the platen (where the paper out sensor is located), the printer will not come on-line. This situation will occur with any printer that does not have the paper out sensor at the left edge of the platen. Solutions: The user can adjust for the paper out sensor by moving the paper to the center of the platen and entering a text adjustment right code to accommodate for the difference. For instance, if the paper was moved 2" to the right to cover the paper out sensor, then a text adjustment of 2" right should be entered (Shift-F8, 2, 7, 5, 9). How/Why: This is really a limitation of the hardware. Different printers have the paper out sensors in different places.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.