DOS Programs And Macintosh Applications Print

DocumentID: 608424
Revision Date: 29-Feb-96 1:33:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Printing envelopes from an IBM/DOS application requires that the envelopes be inserted in the HP LaserJet 4 or HP LaserJet 4M printer stamp edge first (return address edge last). The Macintosh printer driver requires that the envelopes be fed into the printer return address edge first (stamp edge last). Solutions: The HP LaserJet 4/4M printer manual demonstrates that envelopes should be inserted into the printer stamp edge first (return address last). The IBM/DOS printer driver is performing this operation correctly. The Macintosh printer driver is rotating the text in the opposite (reverse) direction. WPCorp currently has no plans to write a special printer driver for IBM/DOS applications to perform this operation incorrectly.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.