HP LaserJet IIP - "Error 22"

DocumentID: 634386
Revision Date: 29-Feb-96 3:03:39 PM

The information in this document applies to:
WordPerfect® 5.0 for DOS

Problem

Solutions: If a customer receives an "Error 22" while printing, try checking their cable. One customer who received this message did not have their cable plugged in tightly. Once it was pushed firmly into place, the error no longer occurred. *This information is a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.