CPT Laser LP6 - QMS Big Kiss - [1:0r Printing

DocumentID: 646678
Revision Date: 29-Feb-96 8:19:16 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: [1:0r was printing on every page when using a CPT Laser LP6 Printer. The customer had the QMS Big Kiss printer defined in WordPerfect. The problem was corrected by changing the XON XOFF to Yes. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.