Printing from Multiple Bins to HP Laserjet 4M

DocumentID: 666543
Revision Date: 29-Feb-96 8:49:56 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Customer was only able to print from the lower bin of the HP LaserJet 4M. She wanted to be able to use the upper bin. Solutions: Customer needed to select the HP LaserJet 4 sheetfeeder and edit the paper sizes. To select the sheetfeeder, from a normal editing screen in WordPerfect press (Shift+F7 Print) | S Select Printer | 3 Edit | 3 Sheetfeeder. Highlight HP LaserJet 4 (SF) and press 1 Select. Finally press F7 to exit back to the document screen. To edit the paper sizes press (Shift+F8) Format | 2 Page | 7 Paper Size/Type. Highlight the paper size that needs to pull from a tray other than the lower tray and press 5 Edit. Now press 5 Location | 2 Bin Number and input the correct bin number and press (enter). Bin settings are: Bin 1 = Upper Cassette Bin 2 = Manual Paper Bin 3 = Manual Envelope Bin 4 = MP Tray Bin 5 = Lower Cassette (Optional) Bin 6 = Auto Envelope Feeder (Optional) Finally, press F7 to exit back to the document screen. Note: The above will also work for the HP Laserjet 4.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.