Star NX-2430 - Entering The Code For A Slashe

DocumentID: 642017
Revision Date: 29-Feb-96 8:18:42 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The code to print a slashed 0 to the Star NX-2430 is <27>~1. The steps below will allow you to add this to the printer driver. 1. Enter PTR and retrieve the .PRS file 2. Highlight the Initialize And Reset, then press Enter 3. Insert the following code at the end of the Initialize At Start Of Print Job line. [27]"~"[1]. To turn Slashed 0 off, use the code [27]"~"[1].

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.