Brother HR-40 - Self Test

DocumentID: 646398
Revision Date: 29-Feb-96 8:19:14 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: To do a self test on the Brother HR-40 printer, hold down the orange SEL button and turn the printer on. The characters on the print wheel will then print. This is a quick way to determine if the print wheel is set correctly in the printer if the printer has been printing garbage.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.