Panasonic KX-P1654 - General Information

DocumentID: 646855
Revision Date: 29-Feb-96 8:19:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Fonts: SLQ, Courier, Prestige, Bold PS, Script, Sans Serif, Orator, Roman, Draft Pica, Draft Elite, and Draft Micron Characters Per Inch: 5, 6, 7.5, 8.5, 10, 12, 15, 17, 20 cpi, and proportional spacing Characters Per Line: 68, 81, 102, 116, 136, 163, 204, 233, and 272 cpi Paper Specifications: Continuous: 4" to 15.5" Single Sheets: 4" to 16.5" Envelopes: #6 and #10 Copies: up to original plus 3 noncarbon copies Thickness: maximum thickness less than 0.013" Paper Feed Paths/Methods: Front (pull tractor adjustable) Rear (push tractor adjustable) Bottom (pull tractor adjustable) Top (single sheets) Interface: Centronics parallel RS-232 serial, optional Compatibility: Epson LQ-1050 IBM Proprinter XL24E

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.