Unisys Model 37 - Configure In HP LaserJet Pl

DocumentID: 646107
Revision Date: 29-Feb-96 8:19:11 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is printing to a Unisys Model 37 printer. They are using the 11/09/90 driver. The customer had to back up their files at DOS and then restore them. After restoring all of the files, everything worked correctly except printing. When printing, the only thing that will print is printer codes. The Standard Printer definition worked fine. Solutions: The Unisys Model 37 printer is supported in the HP LaserJet Plus (+) emulation mode. If the printer is configured this way, there will be no problem. To find out what emulation the printer is currently using, take the printer off-line and press the STATUS button. The current emulation is listed after P1(emulation) in the second column of the Miscellaneous Status section of the Status Sheet. The value for the P1(emulation) should be set at 6 for the HP LaserJet Plus. The emulation mode can be changed at DOS by entering the following at a DOS prompt: copy con lpt1 (or the current port) !R! FRPO P1,n; (where n=emulation. See values below) EXIT; ^Z The values for the n variable are: 1=IBM-PC Graphics Printer 2=Diablo 630 3=Qume Sprint 11 4=NEC Spinwriter 3550 5=Epson FX-80 6=HP LaserJet Plus 7=Unisys Model 31

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.