Dot Pitch Definition

DocumentID: 655821
Revision Date: 29-Feb-96 8:29:38 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Dot pitch: The sharpness of the images that appear on your computer monitor is defined by the dot pitch. Dot pitch measures the width of the dots that make up a pixel. The smaller the dot pitch, the sharper the image. Color monitors use three dots in red, green, and blue (RGB) to focus on a single point or dot to make up a pixel. On monochrome monitors, each dot is a pixel. The accepted standard dot pitch is 31/100 of a millimeter (.31mm).

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.