Star NB24-10 - Printing Broken Graphics Lines

DocumentID: 645900
Revision Date: 29-Feb-96 8:19:09 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: When printing a Double High font with a graphics box around it, the box is broken when printed to the Star NB24-10. Solutions: This is a limitation of the tractor feed mechanism. This is common with all tractor feed printers and is a hardware limitation. Using friction feed instead of tractor feed will correct the problem.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.