Garbage Prints On Tandy DMP 2200 Using IBM Pr

DocumentID: 610197
Revision Date: 29-Feb-96 1:34:28 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Garbage printed when a customer used an IBM Proprinter driver to print to a Tandy DMP 2200 printer. Solutions: If the suggested emulation does not work when you print to the Tandy DMP 2200, check the switch setting for IBM/Tandy and make sure it is set to IBM. Also, when you receive the prompt for WP (Word Processing) or DP (Data Processing) select WP.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.