Epson EPL-7000 Printer Buttons On The Control

DocumentID: 646556
Revision Date: 29-Feb-96 8:19:15 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: There are four arrow buttons on the printer (Up, Down, Left, and Right). The following information discusses use of these buttons and others on the printer. You use the four arrows to select and set printer options in SelecType mode. Their functions are described in detail in Chapter 3 of the Testing and Connecting Your Printer manual. Feed When the printer is off-line and the CH P or CH S light is lit, press this button to print out received data. If you use both channels, you can print data received by either channel. If you press the Up Arrow, Down Arrow, or the On Line button, the printer returns to its previous status without printing data. On Line This switches the printer between on-line and off-line status. This switch is disabled when you are in SelecType mode. Continue This button has three functions, so it has three names, Continue, Copy End, Reset. Continue - This enables the printer to resume printing after some error or maintenance messages. If the Continue light is flashing, read the corresponding error or status message on the display and correct the problem as described in Chapter 7. Copy End - This cancels the remaining copies during multiple-copy printing. This button is effective only when the printer is off-line. Reset - This cancels some settings made with SelecType or software commands. When you hold down this button for several seconds, "Reset" appears on the display and all settings return to their previously saved values. The page being printed when this button is pressed is finished. All remaining data is discarded, however. If you press the Up or Down Arrow, the printer returns to its previous status without printing data. If you continue to hold down this button after "Reset" appears, "Initialize" appears on the display and the printer settings return to the power-on default settings. SelecType Enters or exits SelecType mode. Press once to enter Level 1; hold down to enter Level 2. When you enter each level, the corresponding indicator light goes on.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.