IBM 4019 LaserPrinter E - "Error 2" When Prin

DocumentID: 634415
Revision Date: 29-Feb-96 3:03:40 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer was trying to print envelopes on an IBM 4019 LaserPrinter E with an envelope feeder. Each time the job was sent, they received an "Error 2" on the printer. Their problem was corrected by securing the cable between the printer and the envelope feeder. Apparently, the cable between the two can be easily disconnected.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.