Data Bits Explanation

DocumentID: 655253
Revision Date: 29-Feb-96 8:29:36 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Data Bits: When using serial ports that send data one bit at a time, it is important for the devices at each end to know how many bits make up the actual piece of data. The most common settings are 7 and 8 data bits. This knowledge enables both devices at each end to synchronize. Also see: parity, stop bits, handshaking, XON/XOFF protocol, ETX/ACK protocol.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.