Printer - Not Printing To The End Of Page

DocumentID: 626231
Revision Date: 29-Feb-96 1:41:34 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Problem: The document is not printing to the end of the paper. Possible Solutions: 1. Check the top margin to see if a text adjustment is needed. 2. If using single sheets, check for a small bottom margin. If a small bottom margin is set, the paper will pass the paper out (PO) detector before it has finished printing. In this case, try to disable the paper out detector with a dip switch or menu setting. The customer can determine which switch controls the PO detector by referring to their printer manual. 3. Try testing the printer at DOS by typing the numbers 1, 2, 3, etc., down the page until there are enough numbers to fill one complete page and part of a second page (about 70 lines). Print the test document to determine if there is a blank page between the two pages. 4. Enter the PTR Program and retrieve the .PRS file. Go into Vertical Motion, which is found under Maximum Units, and change the 255 to 35. (This works well on IBM Quietwriter printers.)

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.