Panasonic KX-P4450 And Envelope Tray

DocumentID: 646189
Revision Date: 29-Feb-96 8:19:13 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: With the envelope tray in the lower slot and letter in the upper slot, the top margin prints too low any time an envelope has been printed previously on the Panasonic KX-P4450 printer. The only remedy she has found is to pull out the letter tray and put it back in. This works until another envelope is printed. Using text adjustment only complicates the problem. Her ROM version is 1.01. Solutions: The user needs to make sure that after changing paper trays, they reset the printer. 1. Take the printer off line by pressing the on-line button. 2. Change the paper tray. 3. Press the Reset button and then press the Enter button. This will reset the printer with the new paper tray. 4. Press the on-line button. If the user needs to see if the printer has the new paper size, take the printer off-line and press the Test button then press the Enter button. It will tell them what size form is default.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.