Star NX-2420 - Enabling The Short Tear Off Fe

DocumentID: 646045
Revision Date: 29-Feb-96 8:19:10 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The following changes can be made to the Star NX-2420 (or NX-2420 Rainbow) driver to enable the short tear off feature: 1. Enter the PTR Program 2. Retrieve the .PRS or .ALL file (STNX2420.PRS/WPDM9.ALL or STNX24RA.PRS for the NX-2420 Rainbow) 3. Press Enter on Initialize And Reset 4. Delete the codes that appear on the lines for "Reset At End Of Print Job," "Printer Auto Page Advance," "Eject Page," and "Set Page Length"* 5. Exit and save *In order for the short tear off to work correctly, all codes need to be deleted. Note: Removing these lines will require the customer to turn the printer off and on before using another application, if that application does not reset the printer. If the customer sees problems with another program after leaving WP, the customer should turn the printer off and on. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.