IBM 4029 LaserPrinter 10 PostScript - Auto Sw

DocumentID: 635166
Revision Date: 29-Feb-96 3:03:46 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer requested support for the auto switching feature of the IBM 4029 LaserPrinter 10 PostScript printer in WordPerfect 5.1. There is a printer command called the Set Initial Conditions (SIC) that will switch software emulations, however, WP did not implement this in the PostScript printer definition because the SIC command will delete permanent fonts at the end of the job. This creates a serious limitation if the printer is in PostScript all of the time. Customers may wish to use the Automatic Emulation Switching (AES) utility provided by Lexmark International. Please contact Lexmark International for more information concerning this utility.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.