HP LaserJet III/IIID - Extra FF Before Print

DocumentID: 633955
Revision Date: 29-Feb-96 3:03:29 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: While using either the HP LaserJet III or IIID, print jobs are receiving an extra form feed (FF) command. Solutions: The printer is in landscape mode. Have the customer do the following: 1. Try changing the printer mode to portrait. 2. Try changing the .ALL file in the PTR Program. Enter Initialize And Reset, select Initialize At Start Of Print Job, and on the fifth line down, change [27]"*p3000X" to [27]"*p4500X". Then exit the PTR Program, save, and replace. The customer will then need to update the printer file.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.