HP LaserJet IIID -- Manual Bin 3 Pull From En

DocumentID: 635455
Revision Date: 29-Feb-96 3:03:53 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: A customer had an HP LaserJet IIID, which has two bins, and an envelope feeder, which feeds into the manual feed slot on the upper cassette. The customer wanted to print a legal size page fed manually through the lower cassette, since obviously the upper cassette was being used. However, even though they had a sheet feeder defined and had set the location of the legal form to Bin 3 (the manual feed bin), the printer was pulling the paper from the envelope feeder. Solutions: The HP LaserJet IIID can pull paper manually from either bin when both bins are empty. However, if both bins have paper in them, the printer will pull from the upper cassette by default (thus the print job was pulling from the upper cassette -- see Folio memo WALL_8754B). By changing the Trays setting on the printer (take printer off-line, and press MENU until it reads TRAYS=BOTH*) to TRAYS=LOWER*, the customer was able to get manual paper to default to the lower cassette.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.