Printing Labels On An Epson LQ-950 - Don't Se

DocumentID: 642148
Revision Date: 29-Feb-96 8:18:43 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer wanted to print single column tractor feed labels on an Epson LQ-950 printer. The first two labels would print correctly, but after that it would print one label and skip ten inches. The customer had the Epson LQ-950 SF sheet feeder selected in the Printer Edit screen (Shift F7, S, 3, 3). After the customer selected none for sheet feeder, the labels printed fine.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.