IBM Quietwriter I Not Ejecting Page From Shee

DocumentID: 645089
Revision Date: 29-Feb-96 8:19:03 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is printing a document to the IBM Quietwriter I (Old EPROM) with a single bin sheet feeder. She has selected the sheet feeder and set forms for Location: Bin 1. When the document prints, the page is scrolled up through the sheet feeder but does not completely clear the sheet feeder. Solutions: The IBM Quietwriter I regular and (Old EPROM) have a hardware limitation with the ejecting of the last page of the print job when using a sheet feeder. There is no work around known, except that this was fixed on the IBM Quietwriter II. You can try to do the following, but it usually does not work and is a last resort. If this does not work then there is nothing that we can do to fix the problem. 1. Enter the PTR Program, retrieve the .PRS file, and Enter on the printer name. 2. Press Enter on Initialize and Reset. 3. Move to Printer Auto Page Advance and replace the current command with "Yes." 4. Move to Eject Page (When Not Using Sheet Feeder) and put in a [12].

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.