TI OmniLaser 2106 - Printing Envelopes

DocumentID: 647131
Revision Date: 29-Feb-96 8:19:19 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: When printing envelopes on a TI OmniLaser 2106, the printer displayed a paper error after the print job unless the following changes were made to turn envelopes on and set the tray to Optional Paper. Turning envelopes on 1. Press Setup/Test 2. Press Next until the LED reads Setup on line 2 3. Press Select 4. Press Next until it reads Miscellaneous 5. Press Select 6. Press Next until it reads Envelope 7. Press Select 8. Press Next until it reads On 9. Press Select and put it back on-line Changing the Tray Setting 1. Press Setup/Test 2. Press Next until Setup is displayed 3. Press Select 4. Press Next until it reads Input Tray 5. Press Select 6. Press Next until it reads Optional 7. Press Select and the printer will go back on-line.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.