Print - "Invalid Drive Path Specification" Ca

DocumentID: 651969
Revision Date: 29-Feb-96 8:29:11 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The message "Invalid Drive Path Specification" can appear when printing if an incorrect path (or no path at all) has been specified in the /PF switch. (The /PF startup option is used to redirect the printer overflow files.) If the user is executing WordPerfect from Shell, they may want to verify that the switch is properly defined on the Program Information screen.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.