Epson FX-850 Won't Print Top Margin Less Than

DocumentID: 647650
Revision Date: 29-Feb-96 8:19:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using the Epson FX-850. He is trying to print a top margin of less than 3/8" without any success. We tried offsets, 0" top margins and defining a page as a label, and nothing worked (the smallest top margin we got was 3/8"). Solutions: If the customer is using the auto-load and short tear-off features on the printer, it will always load at that position and cannot really be adjusted. Each time the paper is torn off and the printer returns back to print, it will align at the same position. WP will not back the paper up at any time.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.